{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M9"]
[]
[]
[]
[]
["","","","","","2MXM50M3V1B9","2MXM50M2V1B9"]
["Dimenzije","Uređaj","","Visina","mm","550","550"]
["","","","Širina","mm","765","765"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","285","285"]
["Težina","Uređaj","","","kg","41","41"]
["Motor ventilatora","Brzina","Hlađenje","Superniska","o/min","500","500"]
["","","Grejanje","Superniska","o/min","500","500"]
["Kompresor","Type","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","48","48"]
["","Grejanje","","Visok","dBA","50","50"]
["Rashladni fluid","Tip","","","","R-32","R-32"]
["","Količina","","","kg","1.15","1.15"]
["","Količina","","","tCO2Eq","0.78","0.8"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675.0"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","","20"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 20m)","0,02 (za dužinu cevovoda preko 20m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15.0","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Ukupna duћina cevi","Sistem","Aktuelno","m","30","30"]
["Standardni pribor","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napajanje","Faza","","","","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-230-240","220-230-240"]
["Beleške","","","","","(1) - Za jednu prostoriju","(1) - Svaka klima-komora D-AHU Professional može da se prilagodi vašim potrebama. Odaberite svoj AHU uređaj na internet lokaciji tools.daikinapplied.eu"]