{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Nivo zvučnog pritiska","Grejanje","","Nom.","dBA","48","48","","50","50"]
["","Hlađenje","","Nom.","dBA","47","47","","48","48"]
["Standardni pribor","Priručnik za instalaciju","","","","1","1","","1","1"]
["","Vreća za zavrtnje","","","","1","1","","1","1"]
["","čep ispusnog otvora","","","","1","1","","1","1"]
["","Redukcioni sklop","","","","","","","1","1"]
["Rashladno sredstvo","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Punjenje","","","kg","1.20","1.20","","1.60","1.60"]
["","Type","","","","R-410A","R-410A","","R-410A","R-410A"]
["Cevne spojnice","Razlika nivoa","IU - IU","Maks.","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Maks.","m","15","15","","15","15"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 20m)","0,02 (za dužinu cevovoda preko 20m)","","0,02 (za dužinu cevovoda preko 20m)","0,02 (za dužinu cevovoda preko 20m)"]
["","Ukupna duћina cevi","Sistem","Aktuelno","m","30","30","","30","30"]
["Kompresor","Type","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Dimenzije","Uređaj","","širina","mm","765","765","","765","765"]
["","","","Dubina","mm","285","285","","285","285"]
["","","","Visina","mm","550","550","","550","550"]
["Težina","Uređaj","","","kg","38","38","","42","42"]
["Power supply","Phase","","","","1~","1~","","1~","1~"]
["","Frekvencija","","","Hz","50","50","","50","50"]
["","Napon","","","V","220-240","220-240","","220-240","220-240"]
["Beleške","","","","","(1) - Sadrži fluorisane gasove sa efektom staklene bašte","(1) - Sadrži fluorisane gasove sa efektom staklene bašte","","(1) - Sadrži fluorisane gasove sa efektom staklene bašte","(1) - Sadrži fluorisane gasove sa efektom staklene bašte"]
["Dimenzije","Uređaj","","Visina","mm","","","550","","","550"]
["","","","Širina","mm","","","765","","","765"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","","285","","","285"]
["Težina","Uređaj","","","kg","","","38","","","42"]
["Kompresor","Type","","","","","","Hermetički zatvoren klatni kompresor","","","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","","","10","","","10"]
["","","","Maks.","°CDB","","","46","","","46"]
["","Grejanje","Spolja","Min.","°CWB","","","-15","","","-15"]
["","","","Maks.","°CWB","","","15.5","","","15.5"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","","","47","","","48"]
["","Grejanje","","Nom.","dBA","","","48","","","50"]
["Rashladni fluid","Tip","","","","","","R-410A","","","R-410A"]
["","Količina","","","kg","","","1.20","","","1.60"]
["","Količina","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP (potencijal globalnog otopljavanja)","","","","","","2087.5","","","2087.5"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","","","20","","","20"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","","","0,02 (za dužinu cevovoda preko 20m)","","","0,02 (za dužinu cevovoda preko 20m)"]
["","Razlika nivoa","IU - OU","Maks.","m","","","15","","","15"]
["","","IU - IU","Maks.","m","","","7.5","","","7.5"]
["","Ukupna duћina cevi","Sistem","Aktuelno","m","","","30","","","30"]
["Standardni pribor","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Napajanje","Faza","","","","","","1~","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","","","50","","","50"]
["","Napon","","","V","","","220-240","","","220-240"]
["Standardni pribor","Reducer assembly","","","","","","","","","1"]