{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B","3MXM52N2V1B","3MXM68N2V1B"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Super nisko","m³/min","24","24","24.1"]
["","","Grejanje","Super nisko","m³/min","24","24","24.1"]
["","","","Super nisko","cfm","847","847","851"]
["","","Grejanje","Super nisko","cfm","847","847","851"]
["Dimenzije","Uređaj","","Visina","mm","734","734","734"]
["","","","Širina","mm","958","958","958"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","340","340","340"]
["Težina","Uređaj","","","kg","57","57","62"]
["Motor ventilatora","Brzina","Hlađenje","Superniska","o/min","420","420"]
["","","Grejanje","Superniska","o/min","420","420"]
["Kompresor","Type","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Grejanje","Spolja","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","46","46","48"]
["","Grejanje","","Nom.","dBA","47","47","48"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32"]
["","Količina","","","kg","1.80","1.80","2.00"]
["","Količina","","","tCO2Eq","1.2","1.2","1.4"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675","675"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","25","25","25"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 30m)","0,02 (za dužinu cevovoda preko 30m)","0,02 (za dužinu cevovoda preko 30m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Ukupna duћina cevi","Sistem","Aktuelno","m","50","50","50"]
["Standardni pribor","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240"]
["Standardni pribor","Drain cap","","","","","","3"]
["","Reducer assembly","","","","","","1"]