{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-E"]
[]
[]
[]
[]
["","","","","","4MXS80E3V3B2","4MXS80E3V3B","4MXS80E7V3B"]
["Dimensions","Unit","","Height","mm","770","770"]
["","","","Width","mm","900","900"]
["","","","Depth","mm","320","320"]
["Težina","Uređaj","","","kg","72","72"]
["Compressor","Type","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Grejanje","Spolja","Min.","°CWB","-15","-15"]
["","","","Maks.","°CWB","18","18"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","48","48"]
["","Grejanje","","Nom.","dBA","49","49"]
["Rashladno sredstvo","Tip","","","","R-410A","R-410A"]
["","Punjenje","","","kg","2.99","2.99"]
["","GWP","","","","2,087.5","2,087.5"]
["Povezivanje cevi","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 30m)","0,02 (za dužinu cevovoda preko 30m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Ukupna duћina cevi","Sistem","Aktuelno","m","70","70"]
["Standardni pribor","Priručnik za instalaciju","","","","1","1"]
["","čep ispusnog otvora","","","","1","1"]
["","Redukcioni sklop","","","","1","1"]
["Power supply","Phase","","","","1~","1~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","230","230"]
["Beleške","","","","","(1) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 7,5m","(1) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 7,5m"]
["","","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m"]
["","","","","","(3) - Sadrži fluorisane gasove sa efektom staklene bašte","(3) - Sadrži fluorisane gasove sa efektom staklene bašte"]
["Dimenzije","Uređaj","","Visina","mm","","","770"]
["","","","Širina","mm","","","900"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","","320"]
["Težina","Uređaj","","","kg","","","72"]
["Compressor","Type","","","","","","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["","Grejanje","Spolja","Min.","°CWB","","","-15"]
["","","","Maks.","°CWB","","","15.5"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","","","48"]
["","Grejanje","","Nom.","dBA","","","49"]
["Rashladni fluid","Tip","","","","","","R-410A"]
["","Količina","","","kg","","","2.99"]
["","Količina","","","tCO2Eq","","","6.2"]
["","GWP (potencijal globalnog otopljavanja)","","","","","","2087.5"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","","","25"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","","","0,02 (za dužinu cevovoda preko 30m)"]
["","Razlika nivoa","IU - OU","Maks.","m","","","15"]
["","","IU - IU","Maks.","m","","","7.5"]
["","Ukupna duћina cevi","Sistem","Aktuelno","m","","","70"]
["Standardni pribor","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Napajanje","Faza","","","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","","","50"]
["","Napon","","","V","","","230"]