{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Dimenzije","Uređaj","","Visina","mm","734","734"]
["","","","Širina","mm","1,040","1,040"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","408","408"]
["Težina","Uređaj","","","kg","69","73"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","48","52"]
["","Grejanje","","Nom.","dBA","49","53"]
["Rashladni fluid","Tip","","","","R-32","R-32"]
["","Količina","","","kg","2","2.4"]
["","Količina","","","tCO2Eq","1.35","1.62"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","25 (2)","25 (3)"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 30m)","0,02 (za dužinu cevovoda preko 30m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15 (3)","15"]
["","","IU - IU","Maks.","m","7.5 (3)","7.5 (3)"]
["","Ukupna duћina cevi","Sistem","Aktuelno","m","60","75"]
["Standardni pribor","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Napajanje","Faza","","","","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-440","220-240"]
["Beleške","","","","","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","","(2) - Za jednu prostoriju","(2) - Za jednu prostoriju"]
["","","","","","(3) - Za jednu prostoriju (za kombinaciju sa FBA71/100/125 i EKHWET i CKHWS pogledati priručnik za instalaciju)","(3) - Za jednu prostoriju (za kombinaciju sa FBA71/100/125 i EKHWET i CKHWS pogledati priručnik za instalaciju)"]
["","","","","","(4) - Sadrži fluorisane gasove sa efektom staklene bašte","(4) - Sadrži fluorisane gasove sa efektom staklene bašte"]