{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-A8"]
[]
[]
[]
[]
["","","","","","5MXM90A2V1B8"]
["Dimenzije","Uređaj","","Visina","mm","734"]
["","","","Širina","mm","974"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","408"]
["Težina","Uređaj","","","kg","68"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","52"]
["","Grejanje","","Nom.","dBA","52"]
["Rashladni fluid","Tip","","","","R-32"]
["","Količina","","","kg","2.40"]
["","Količina","","","tCO2Eq","1.62"]
["","GWP (potencijal globalnog otopljavanja)","","","","675"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","25 (1)"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 30m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15"]
["","","IU - IU","Maks.","m","7.5"]
["","Ukupna duћina cevi","Sistem","Aktuelno","m","75"]
["Standardni pribor","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Opseg energetske efikasnosti","","","","","A+++ ~ D"]
["Napajanje","Faza","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-240"]
["Beleške","","","","","(1) - Za jednu prostoriju"]
["","","","","","(2) - Za kombinaciju sa CVXM-A, FVXM-A - maksimalna dužina cevovoda je 30 m."]
["","","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["","","","","","(5) - Sadrži fluorisane gasove sa efektom staklene bašte"]