{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Kapacitet hlađenja","Nom.","","kW","9.5","12.1 (1)"]
["Hlađenje prostora","SEER","","","4.65","4.68"]
["","Godišnja potrošnja električne energije","","kWh/a","716","1,550"]
["","Kapacitet","Pdesign","kW","9.50","12.1"]
["","Klasa energetske efikasnosti","","","B"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Klasa energetske efikasnosti","","","A"]
["","Godišnja potrošnja električne energije","","kWh/a","2,498","3,340"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","1,813"]
["","EER","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Direktiva o energetskom označavanju","Hlađenje","","D"]
["","","Grejanje","","B"]
["Kapacitet grejanja","Nom.","","kW","10.8","13.5 (2)"]
["Beleške","","","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m"]
["","","","","(2) - Godišnja potročnja energije je u skladu sa direktivom o energetskom označavanju 2002/31/EC","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m"]
["","","","","(3) - SEER i SCOP su u skladu sa EN 14825","(3) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["","","","","(4) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]