{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-C / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ACQ71CV1 / AZQS71B2V1B","ACQ100CV1 / AZQS100B8V1B","ACQ125CV1 / AZQS125B8V1B"]
["Kapacitet hlađenja","Nom.","","kW","6.8","9.5","12.1"]
["Hlađenje prostora","SEER","","","4.65","4.65"]
["","Godišnja potrošnja električne energije","","kWh/a","512","716"]
["","Kapacitet","Pdesign","kW","6.80","9.50"]
["","Klasa energetske efikasnosti","","","B","B"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","6.33","7.60"]
["","SCOP/A","","","3.80","3.80"]
["","Klasa energetske efikasnosti","","","A","A"]
["","Godišnja potrošnja električne energije","","kWh/a","2,332","2,800"]
["Nominalna efikasnost","Annual energy consumption","","kWh","1,025","1,480","2,010"]
["","EER","","","3.31","3.21","3.01"]
["","COP","","","3.61","3.61","3.41"]
["","Direktiva o energetskom označavanju","Hlađenje","","B","A"]
["","","Grejanje","","A","A"]
["Kapacitet grejanja","Nom.","","kW","7.50","10.80","13.5"]
["Beleške","","","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["","","","","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]