{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Nečujan rad","dBA","","36","","41"]
["","","","Nizak","dBA","","38","","43"]
["","Hlađenje","","Nečujan rad","dBA","","36","","41"]
["","","","Nizak","dBA","","38","","43"]
["","","","Visok","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Standardni pribor","Priručnik za instalaciju","","","","","Priručnik za instalaciju","","Priručnik za instalaciju"]
["","Priručnik za upotrebu","","","","","Priručnik za upotrebu","","Priručnik za upotrebu"]
["","Navoji","","","","","Navoji","","Navoji"]
["","Podloška","","","","","Podloška","","Podloška"]
["","Bežični daljinski upravljač","","","","","Bežični daljinski upravljač","","Bežični daljinski upravljač"]
["","Zaštitna rešetka","","","","","Zaštitna rešetka","","Zaštitna rešetka"]
["","Baterija","","","","","Baterija","","Baterija"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Piping connections","Tečnost","","SP","mm","","9.52","","9.52"]
["","Gas","","SP","mm","","15.88","","15.88"]
["","Ispusni otvor","","","","","19.05","","19.05"]
["Apsorbovana snaga","Hlađenje","","Nom.","kW","","0.094","","0.137"]
["","Grejanje","","Nom.","kW","","0.094","","0.137"]
["Nivo zvučne snage","Hlađenje","","","dBA","","56","","60"]
["","Grejanje","","","dBA","","56","","60"]
["Dimenzije","Uređaj","","Širina","mm","","820","","820"]
["","","","Dubina","mm","","820","","820"]
["","","","Visina","mm","","300","","300"]
["Kućište","Materijal","","","","","Galvanizovani čelik","","Galvanizovani čelik"]
["Težina","Uređaj","","","kg","","39","","39"]
["Ventilator","Brzina protoka vazduha","Grejanje","Visok","m³/min","","29.2","","34.0"]
["","","","Nizak","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Hlađenje","Nizak","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Visok","m³/min","","29.2","","34.0"]
["","","","Nečujan rad","m³/min","","17.6","","22.1"]
["","","Hlađenje","Nečujan rad","m³/min","","17.6","","22.1"]
["Ukrasna maska","Težina","","","kg","","4","","4"]
["","Dimenzije","","Visina","mm","","82","","82"]
["","","","Dubina","mm","","990","","990"]
["","","","Širina","mm","","990","","990"]
["","Boja","","","","","Bela","","Bela"]
["Power supply","Phase","","","","","1~","","1~"]
["","Ime","","","","","V1","","V1"]
["","Frekvencija","","","Hz","","50","","50"]
["","Napon","","","V","","220-240","","220-240"]
["Ventilator","Brzina protoka vazduha","Grejanje","Nečujan rad","m³/min","15","","22.1"]
["Ulazna snaga","Grejanje","","Nom.","kW","0.067","","0.137"]
["","Hlađenje","","Nom.","kW","0.067","","0.137"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Nečujan rad","m³/min","15","","22.1"]
["Kućište","Materijal","","","","Galvanizovani čelik","","Galvanizovani čelik"]
["Dimenzije","Uređaj","","Visina","mm","265","","300"]
["","","","Širina","mm","820","","820"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","820","","820"]
["Težina","Uređaj","","","kg","31","","39"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Nizak","m³/min","17.6","","26.3"]
["","","Grejanje","Visok","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Nizak","m³/min","17.6","","26.3"]
["Nivo zvučne snage","Hlađenje","","","dBA","54","","60"]
["","Grejanje","","","dBA","54","","60"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Nizak","dBA","35","","43"]
["","","","Nečujan rad","dBA","32","","41"]
["","Grejanje","","Visok","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Nizak","dBA","35","","43"]
["","","","Nečujan rad","dBA","32","","41"]
["Povezivanje cevi","Tečnost","","SP","mm","9.52","","9.52"]
["","Gas","","SP","mm","15.88","","15.88"]
["","Ispusni otvor","","","","19.05","","19.05"]
["Ukrasna maska","Dimenzije","","Visina","mm","82","","82"]
["","","","Širina","mm","990","","990"]
["","","","Dubina","mm","990","","990"]
["","Težina","","","kg","4","","4"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","ARCWLA","","ARCWLA"]
["","Žičani daljinski upravljač","","","","ARCWB","","ARCWB"]
["Standardni pribor","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Napajanje","Faza","","","","1~","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","","50"]
["","Napon","","","V","220-240","","220-240"]