{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEA100A2VEB / AZQS100B8V1B","ADEA125A2VEB / AZQS125B8V1B"]
["Kapacitet hlađenja","Nom.","","kW","9.50","12.10"]
["Hlađenje prostora","SEER","","","5.10","4.83"]
["","Godišnja potrošnja električne energije","","kWh/a","652","1,504"]
["","Kapacitet","Pdesign","kW","9.50","12.10"]
["","Klasa energetske efikasnosti","","","A"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","7.60","7.93"]
["","SCOP/A","","","3.81","3.50"]
["","Klasa energetske efikasnosti","","","A"]
["","Godišnja potrošnja električne energije","","kWh/a","2,793","3,167"]
["Nominalna efikasnost","EER","","","","2.27"]
["Kapacitet grejanja","Nom.","","kW","10.80","13.50"]
["Beleške","","","","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["","","","","(3) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m","(3) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m"]
["","","","","(4) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m","(4) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m"]