{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEQ71C2VEB / AZQS71B2V1B","ADEQ100C2VEB / AZQS100B8V1B","ADEQ125C2VEB / AZQS125B8V1B"]
["Kapacitet hlađenja","Nom.","","kW","","9.50 (1)","12.1 (1)"]
["Hlađenje prostora","SEER","","","","5.10","4.71"]
["","Godišnja potrošnja električne energije","","kWh/god.","","652","1,543"]
["","Kapacitet","Pdesign","kW","","9.50","12.1"]
["","Klasa energetske efikasnosti","","","","A"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","","7.60","7.93"]
["","SCOP/A","","","","3.81","3.50"]
["","Klasa energetske efikasnosti","","","","A"]
["","Godišnja potrošnja električne energije","","kWh/god.","","2,793","3,167"]
["Nominalna efikasnost","EER","","","","","2.27"]
["Kapacitet grejanja","Nom.","","kW","","10.8 (2)","13.5 (2)"]
["Beleške","","","","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m"]
["","","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m"]
["Opseg energetske efikasnosti","","","","A+++ ~ D"]