{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-A"]
[]
[]
[]
[]
["","","","","","ARXM25A5V1B","ARXM35A5V1B","ARXM50A5V1B","ARXM60A5V1B","ARXM71A5V1B"]
["Dimenzije","Uređaj","","Visina","mm","610","610","734","734","734"]
["","","","Širina","mm","923","923","954","954","954"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","367","367","401","401","401"]
["Težina","Uređaj","","","kg","36","36","49","49","49"]
["Motor ventilatora","Brzina","Hlađenje","Superniska","o/min","600","600","500"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","50","50","50 (1), 46 (1)","46","46"]
["","Grejanje","Spolja","Min.","°CWB","-21","-21","-21 (1), -15 (1)","-15","-15"]
["","","","Maks.","°CWB","18","18","18","18","18"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","46","47","48","48","52"]
["","Grejanje","","Nom.","dBA","47","49","49","49","52"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32","R-32","R-32"]
["","Količina","","","kg","0.95","0.95","1.1","1.15","1.15"]
["","Količina","","","tCO2Eq","0.65","0.65","0.75","0.78","0.78"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675","675","675","675"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","20","20","30","30","30"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","002 (za dužinu cevovoda preko 10m)","002 (za dužinu cevovoda preko 10m)","002 (za dužinu cevovoda preko 10m)","002 (za dužinu cevovoda preko 10m)","0035 (za dužinu cevovoda preko 10 m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15","15","20","20","20"]
["Standardni pribor","Installation manual","","","","1","1","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","1","3","3"]
["Opseg energetske efikasnosti","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240","220-240"]
["Beleške","","","","","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["","","","","","(3) - Sadrži fluorisane gasove sa efektom staklene bašte","(3) - Sadrži fluorisane gasove sa efektom staklene bašte","(3) - Sadrži fluorisane gasove sa efektom staklene bašte","(3) - Sadrži fluorisane gasove sa efektom staklene bašte","(3) - Sadrži fluorisane gasove sa efektom staklene bašte"]
["Standardni pribor","ARXM50A5V1B","","","","","","1"]
["","Drain plug","","","","","","","1","1"]