{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-N9"]
[]
[]
[]
[]
["","","","","","ARXM25N2V1B9","ARXM25N5V1B9","ARXM35N5V1B9","ARXM35N2V1B9","ARXM50N2V1B9","ARXM60N2V1B9","ARXM71N2V1B9"]
["Dimenzije","Uređaj","","Visina","mm","550","550","550","550","734","734","734"]
["","","","Širina","mm","765","765","765","765","870","870","870"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","285","285","285","285","373","373","373"]
["Težina","Uređaj","","","kg","32","32","32","32","50","50.0","50.0"]
["Compressor","Tip","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","","-10","-10","","-10","-10","-10"]
["","","","Maks.","°CDB","","50","50","","50","46","46"]
["","Grejanje","Spolja","Min.","°CWB","","-21","-21","","-21","-15","-15"]
["","","","Maks.","°CWB","","18","18","","18","18","18"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","46","46","49","49","48","48","52"]
["","Grejanje","","Nom.","dBA","47","47","49","49","49","49","52"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Količina","","","kg","0.76","0.76","0.76","0.76","1.15","1.15","1.15"]
["","Količina","","","tCO2Eq","0.52","0.52","0.52","0.52","0.78","0.78","0.78"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675","675","675","675","675","675"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","20","20","20","20","30","30","30"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,020 (za dužinu cevovoda preko 10m)","0,035 (za dužinu cevovoda preko 10 m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15","15","15","15","20","20","20"]
["Standardni pribor","Installation manual","","","","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardni pribor","Drain cap","","","","","","","","3","3","3"]
["Kompresor","Tip","","","","","","","","","","Hermetički zatvoren klatni kompresor"]