{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Nivo zvučnog pritiska","Grejanje","","Nom.","dBA","","49.0"]
["","Hlađenje","","Nom.","dBA","","49.0"]
["Standardni pribor","čep ispusnog otvora","","","","","1"]
["","Priručnik za instalaciju","","","","","1"]
["","Oznaka punjenja rashladnog fluida","","","","","1"]
["","Oznake F-gasova sa efektom staklene bašte","","","","","1"]
["","Opšta upozorenja u vezi sa bezbednošću","","","","","1"]
["Rashladno sredstvo","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Charge","","","kg","","0.76"]
["","Tip","","","","","R-32"]
["Radni opseg","Hlađenje","Spolja","Maks.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Cevne spojnice","Razlika nivoa","IU - OU","Maks.","m","","15"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","","0,02 (za dužinu cevovoda preko 10m)"]
["Kompresor","Tip","","","","","Hermetički zatvoren klatni kompresor"]
["Dimenzije","Uređaj","","Širina","mm","","840"]
["","","","Dubina","mm","","350"]
["","","","Visina","mm","","552"]
["Težina","Uređaj","","","kg","","32"]
["Power supply","Faza","","","","","1~"]
["","Frekvencija","","","Hz","","50"]
["","Napon","","","V","","220-240"]
["Beleške","","","","","(1) - Moguće samo u kombinaciji sa ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Sadrži fluorisane gasove sa efektom staklene bašte"]
["","","","","","(2) - Moguće samo u kombinaciji sa ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","","","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["","","","","","","(4) - Moguće samo u kombinaciji sa ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Moguće samo u kombinaciji sa ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Dimenzije","Uređaj","","Visina","mm","552"]
["","","","Širina","mm","840"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","350"]
["Težina","Uređaj","","","kg","32"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50 (4), 46 (5)"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","46.0"]
["","Grejanje","","Nom.","dBA","47.0"]
["Rashladni fluid","Količina","","","kg","0.76"]
["","Količina","","","tCO2Eq","0.52"]
["","GWP (potencijal globalnog otopljavanja)","","","","675"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","20"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 10m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15"]
["Standardni pribor","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Izvor napajanja","Frekvencija","","","Hz","50"]