{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXP-K3"]
[]
[]
[]
[]
["","","","","","ARXP20K3V1B","ARXP25K3V1B","ARXP35K3V1B"]
["Dimenzije","Uređaj","","Visina","mm","550","550","550"]
["","","","Širina","mm","765","765","765"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","285","285","285"]
["Težina","Uređaj","","","kg","32","32","32"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","46","46","48"]
["","Grejanje","","Visok","dBA","47","47","48"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32"]
["","Količina","","","kg","0.76","0.76","0.76"]
["","Količina","","","tCO2Eq","0.52","0.52","0.52"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675","675"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","20.0","20.0","20.0"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15.0","15.0","15.0"]
["Standardni pribor","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240"]