{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXP-N"]
[]
[]
[]
[]
["","","","","","ARXP20N5V1B","ARXP25N5V1B","ARXP35N5V1B"]
["Dimenzije","Uređaj","","Visina","mm","556","556","556"]
["","","","Širina","mm","740","740","740"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","343","343","343"]
["Težina","Uređaj","","","kg","24","24","24"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","48","48","48"]
["","Grejanje","Spolja","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","46","46","48"]
["","Grejanje","","Visok","dBA","47","47","48"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32"]
["","Količina","","","kg","0.55","0.55","0.70"]
["","Količina","","","tCO2Eq","0.37","0.37","0.48"]
["","GWP (potencijal globalnog otopljavanja)","","","","675.0","675.0","675.0"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","20","20","20"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)"]
["","Razlika nivoa","IU - OU","Maks.","m","12","12","12"]
["Standardni pribor","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240"]