{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","","","47","48"]
["","","","Nom.","dBA","","52","","","49"]
["","Hlađenje","","Visok","dBA","","","46","48"]
["","","","Nom.","dBA","","52","","","49"]
["Standardni pribor","čep ispusnog otvora","","","","","1","1","1","1"]
["","Priručnik za instalaciju","","","","","1","1","1","1"]
["Rashladno sredstvo","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Punjenje","","","kg","","1.70","1.0","1.2","1.50"]
["","Tip","","","","","R-410A","R-410A","R-410A","R-410A"]
["Motor ventilatora","Brzina","Hlađenje","Superniska","Obrta/min","","","780","780"]
["","","Grejanje","Superniska","Obrta/min","","","740","740"]
["Radni opseg","Hlađenje","Spolja","Maks.","°CDB","","46","46","46","46"]
["","","","Min.","°CDB","","-10","10","10","-10"]
["","Grejanje","Spolja","Maks.","°CWB","","18","18","18","18"]
["","","","Min.","°CWB","","-15","-15","-15","-15"]
["Povezivanje cevi","Razlika nivoa","IU - OU","Maks.","m","","20.0","15","15","20.0"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)"]
["Nivo zvučne snage","Hlađenje","","","dBA","","65","","","62"]
["","Grejanje","","","dBA","","65","","","62"]
["Kompresor","Tip","","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Dimenzije","Uređaj","","Width","mm","","825","765","765","825"]
["","","","Depth","mm","","300","285","285","300"]
["","","","Height","mm","","735","550","550","735"]
["Težina","Unit","","","kg","","47","34","34","47"]
["Ventilator","Brzina protoka vazduha","Grejanje","Super nisko","cfm","","","904","904"]
["","","","Super nisko","m³/min","","","25.6","25.6"]
["","","Hlađenje","Super nisko","m³/min","","","30.1","30.1"]
["","","","Super nisko","cfm","","","1,063","1,063"]
["Power supply","Phase","","","","","1~","1~","1~","1~"]
["","Frekvencija","","","Hz","","50","50","50","50"]
["","Napon","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Beleške","","","","","(1) - 220V","","(1) - Pri povezivanju sa višestrukom spoljnom jedinicom, pogledajte specifikacije za tu višestruku spoljnu jedinicu.","(1) - Pri povezivanju sa višestrukom spoljnom jedinicom, pogledajte specifikacije za tu višestruku spoljnu jedinicu."]
["","","","","","(2) - 230V","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","","(3) - 230V","(3) - 230V"]
["","","","","","","","(4) - 240V","(4) - 240V"]
["","","","","","","","(5) - Sadrži fluorisane gasove sa efektom staklene bašte","(5) - Sadrži fluorisane gasove sa efektom staklene bašte"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Super nisko","m³/min","48.9"]
["","","Grejanje","Super nisko","m³/min","43.1"]
["","","","Super nisko","cfm","1727"]
["","","Grejanje","Super nisko","cfm","1522"]
["Dimenzije","Uređaj","","Visina","mm","735"]
["","","","Širina","mm","825"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","300"]
["Težina","Uređaj","","","kg","47"]
["Motor ventilatora","Brzina","Hlađenje","Superniska","Obrta/min","670"]
["","","Grejanje","Superniska","Obrta/min","670"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","10"]
["","","","Maks.","°CDB","46"]
["","Grejanje","Spolja","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","48"]
["","Grejanje","","Visok","dBA","48"]
["Rashladni fluid","Tip","","","","R-410A"]
["","Količina","","","kg","1.7"]
["","Količina","","","tCO2Eq","3.5"]
["","GWP (potencijal globalnog otopljavanja)","","","","2087.5"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","30"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 10m)"]
["","Razlika nivoa","IU - OU","Maks.","m","20"]
["Standardni pribor","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Napajanje","Faza","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-240"]
["Standardni pribor","Oznake F-gasova sa efektom staklene bašte","","","","","1","1","","1"]
["","Oznaka punjenja rashladnog fluida","","","","","1","1","","1"]
["Beleške","","","","","","(1) - Sadrži fluorisane gasove sa efektom staklene bašte","","","(1) - Sadrži fluorisane gasove sa efektom staklene bašte"]