{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS35L3V1B","ARXS25L3V1B (Archived)"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","48"]
["","","","Nizak","dBA","45"]
["Standardni pribor","1","","","","550"]
["Rashladno sredstvo","Punjenje","","","kg","2.5"]
["","Tip","","","","1.2"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Super nisko","m³/min","30.1"]
["","","","Super nisko","cfm","1,063"]
["Motor ventilatora","Brzina","Hlađenje","Superniska","o/min","740"]
["","","Grejanje","Superniska","o/min","-15"]
["Radni opseg","Grejanje","Spolja","Min.","°CWB","20"]
["","","","Maks.","°CWB","10"]
["Nivo zvučnog pritiska","Hlađenje","","Nizak","dBA","44"]
["","","","Visok","dBA","48"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor"]
["Dimenzije","Uređaj","","Širina","mm","285"]
["","","","Dubina","mm","612"]
["","","","Visina","mm","765"]
["Težina","Uređaj","","","kg","34"]
["Ventilator","Brzina protoka vazduha","Grejanje","Super nisko","cfm","904"]
["","","","Super nisko","m³/min","25.6"]
["Power supply","Faza","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-240"]
["Beleške","","","","","(1) - Sadrži fluorisane gasove sa efektom staklene bašte","(1) - 220V"]
["","","","","","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 230V","(3) - 240V"]
["","","","","","(4) - 240V"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Super nisko","m³/min","","30.1"]
["","","Grejanje","Super nisko","m³/min","","25.6"]
["","","","Super nisko","cfm","","1063"]
["","","Grejanje","Super nisko","cfm","","904"]
["Dimenzije","Uređaj","","Visina","mm","","550"]
["","","","Širina","mm","","765"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","285"]
["Težina","Uređaj","","","kg","","34"]
["Motor ventilatora","Brzina","Hlađenje","Superniska","o/min","","780"]
["","","Grejanje","Superniska","o/min","","740"]
["Kompresor","Tip","","","","","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","","10"]
["","","","Maks.","°CDB","","46"]
["","Grejanje","Spolja","Min.","°CWB","","-15"]
["","","","Maks.","°CWB","","18"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","","46"]
["","Grejanje","","Visok","dBA","","47"]
["","","","Nizak","dBA","","44"]
["Rashladni fluid","Tip","","","","","R-410A"]
["","Količina","","","kg","","1.0"]
["","Količina","","","tCO2Eq","","2.1"]
["","GWP (potencijal globalnog otopljavanja)","","","","","2087.5"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","","20"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","","0,02 (za dužinu cevovoda preko 10m)"]
["","Razlika nivoa","IU - OU","Maks.","m","","15"]
["Standardni pribor","Installation manual","","","","","1"]
["","Refrigerant charge label","","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1"]
["","Drain plug","","","","","1"]
["Napajanje","Faza","","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","","50"]
["","Napon","","","V","","220-240"]