{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":11,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXC-B"]
[]
[]
[]
[]
["","","","","","ATXC20BV1B","ATXC25BV1B","ATXC35BV1B","ATXC50BV1B","ATXC60BV1B","ATXC71BV1B"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.6","0.775","1.06","1.57","1.915","2.41"]
["","Grejanje","","Nom.","kW","0.67","0.755","1.075","1.515","1.725","2.49"]
["Kućište","Boja","","","","Bela","Bela","Bela","Bela","Bela","Bela"]
["","Materijal","","","","Polistiren otporan na udar","Polistiren otporan na udar","Polistiren otporan na udar","Polistiren otporan na udar","Polistiren otporan na udar","Polistiren otporan na udar"]
["Dimenzije","Uređaj","","Visina","mm","288","288","288","288","297","297"]
["","","","Širina","mm","785","785","785","785","1005","1005"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","250","250","250","250","288","288"]
["Težina","Uređaj","","","kg","9","9","9.5","9.5","13","13"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","10.8","10.8","10.8","12.2","20.4","20.4"]
["","","","Srednji","m³/min","8.8","8.8","9.1","10.2","15.9","15.9"]
["","","","Nizak","m³/min","6.5","6.5","6.5","8.2","13.6","13.6"]
["","","","Nečujan rad","m³/min","5.4","5.4","5.4","7.4","10.2","10.2"]
["Nivo zvučne snage","Hlađenje","","","dBA","54","54","55","57","60","60"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","38","38","39","45","46","46"]
["","","","Srednji","dBA","33","33","34","39","42","42"]
["","","","Nizak","dBA","26","26","26","33","38","38"]
["","","","Nečujan rad","dBA","20","20","21","29","30","30"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","SP","mm","9.52","9.52","9.52","12.7","12.7","12.7"]
["","Ispusni otvor","","","","16.5","16.5","16.5","16.5","16.5","16.5"]
["Napajanje","Ime","","","","V1","V1","V1","V1","V1","V1"]
["","Faza","","","","1~","1~","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]