{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":9,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-M / ARXM-N9"]
[]
[]
[]
[]
["","","","","ATXM25M2V1B / ARXM25N5V1B9","ATXM25M2V1B / ARXM25N2V1B9","ATXM35M2V1B / ARXM35N5V1B9","ATXM35M2V1B / ARXM35N2V1B9","ATXM50M2V1B / ARXM50N2V1B9"]
["Kapacitet hlađenja","Min.","","kW","1.3","1.3","1.4","","1.70"]
["","Maks.","","kW","3.2","3.2","4.0","","5.30"]
["","Nom.","","kW","2.5","2.5","3.4","","5.00"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","285","285","415"]
["","EER","","","4.39","4.39","4.09","","3.45"]
["","COP","","","5.00","5.00","4.04","","3.79"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","A","","A"]
["","","Grejanje","","A","A","A","","A"]
["Kapacitet grejanja","Nom.","","kW","2.80","2.80","4.00","","5.80"]
["","Min.","","kW","1.30","1.30","1.40","","1.70"]
["","Maks.","","kW","4.70","4.70","5.20","","6.50"]
["Beleške","","","","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["","","","","(2) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(2) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(2) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","","(2) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(3) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(3) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(3) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","","(3) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["Spoljni uređaj","","","","","","","ARXM35N2V1B9"]
["Kapacitet hlađenja","Min.","","kW","","","","1.4"]
["","Nom.","","kW","","","","3.4"]
["","Maks.","","kW","","","","4.0"]
["Kapacitet grejanja","Min.","","kW","","","","1.40"]
["","Nom.","","kW","","","","4.00"]
["","Maks.","","kW","","","","5.20"]
["Nominalna efikasnost","EER","","","","","","4.09"]
["","COP","","","","","","4.04"]
["","Godišnja potrošnja električne energije","","kWh","","","","415"]
["","Direktiva o energetskom označavanju","Hlađenje","","","","","A"]
["","","Grejanje","","","","","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","","","","A+++"]
["","Kapacitet","Pdesign","kW","","","","3.40"]
["","SEER","","","","","","8.50"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","140"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","","","","A+++"]
["","Kapacitet","Pdesign","kW","","","","2.50"]
["","SCOP/A","","","","","","5.10"]
["","Pdh Kapacitet grejanja na -10°C","","kW","","","","2.35"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","686"]
["Opseg energetske efikasnosti","","","","","","","A+++ ~ D"]