{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B9","ATXP25N5V1B9","ATXP35N5V1B9"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.019","0.020","0.032"]
["","Grejanje","","Nom.","kW","0.023","0.023","0.032"]
["Kućište","Boja","","","","Bela","Bela","Bela"]
["Dimenzije","Uređaj","","Visina","mm","286","286","286"]
["","","","Širina","mm","770","770","770"]
["","","","Dubina","mm","225","225","225"]
["Težina","Uređaj","","","kg","8.50","8.50","9.00"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","9.5","9.7","11.5"]
["","","","Srednji","m³/min","7.4","7.7","8.3"]
["","","","Nizak","m³/min","5.6","5.8","6.3"]
["","","","Nečujan rad","m³/min","4.2","4.2","4.5"]
["","","Grejanje","Visok","m³/min","10.4","10.4","11.5"]
["","","","Srednji","m³/min","8.1","8.1","9.0"]
["","","","Nizak","m³/min","6.2","6.4","7.0"]
["","","","Nečujan rad","m³/min","5.2","5.2","5.1"]
["Nivo zvučne snage","Hlađenje","","","dBA","55","55","58"]
["","Grejanje","","","dBA","55","55","58"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","39","40","43"]
["","","","Srednji","dBA","33","33","34"]
["","","","Nizak","dBA","25","26","27"]
["","","","Nečujan rad","dBA","19","19","20"]
["","Grejanje","","Visok","dBA","39","40","40"]
["","","","Srednji","dBA","34","34","35"]
["","","","Nizak","dBA","28","28","29"]
["","","","Nečujan rad","dBA","21","21","21"]
["Povezivanje cevi","Tečnost","","SP","mm","6","6","6"]
["","Gas","","SP","mm","9.50","9.50","9.50"]
["","Ispusni otvor","","","","18","18","18"]
["Kontrolni sistemi","Infrared remote control","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Žičani daljinski upravljač","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardni pribor","Priručnik za instalaciju","","","","1","1","1"]
["","Priručnik za upotrebu","","","","1","1","1"]
["","Infracrveni daljinski upravljač","","","","1","1","1"]
["","AAA suve baterije","","","","2","2","2"]
["","Držač daljinskog upravljača","","","","1","1","1"]
["","Noseća ploča","","","","1","1","1"]
["","Titanijumapatitski dezodorišući filter","","","","1","1","1"]
["","Srebrni filter za prašinu","","","","1","1","1"]
["","Pričvrsni zavrtnji unutrašnje jedinice","","","","2","2","2"]
["","Opšta upozorenja u vezi sa bezbednošću","","","","1","1","1"]
["Power supply","Faza","","","","1~","1~","1~"]
["","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240"]
["Beleške","","","","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m"]
["","","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m (po horizontali)","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m (po horizontali)","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m (po horizontali)"]
["","","","","","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]