{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXTP-K / ARXTP-R"]
[]
[]
[]
[]
["","","","","ATXTP25K3V1B / ARXTP25R2V1B","ATXTP35K3V1B / ARXTP35R2V1B"]
["Kapacitet hlađenja","Min.","","kW","0.80","0.80"]
["","Maks.","","kW","4.40","4.40"]
["","Nom.","","kW","2.50","3.50"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","285","467"]
["","EER","","","4.38","3.75"]
["","COP","","","4.90","4.39"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","A","A"]
["Kapacitet grejanja","Nom.","","kW","3.20","4.00"]
["","Min.","","kW","1.20","1.20"]
["","Maks.","","kW","6.00","6.50"]
["Beleške","","","","(1) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(1) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(2) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(2) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]