{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":9,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MV1"]
[]
[]
[]
[]
["","","","","","AZAS71M2V1B","AZAS100M7V1B","AZAS125M7V1B","AZAS140M7V1B"]
["Dimenzije","Uređaj","","Visina","mm","770","990","990","990"]
["","","","Širina","mm","900","940","940","940"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","320","320","320","320"]
["Težina","Uređaj","","","kg","60","70","70","78"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-5","-5","-5","-5"]
["","","","Maks.","°CDB","46","46","46","46"]
["","Grejanje","Spolja","Min.","°CWB","-15","-15","-15","-15"]
["","","","Maks.","°CWB","15.5","15.5","15.5","15.5"]
["Nivo zvučne snage","Hlađenje","","","dBA","65","70","71","73"]
["","Grejanje","","","dBA","","","71 (1)","73 (1)"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","46","53","53","54"]
["","Grejanje","","Nom.","dBA","47","57","57","57"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32","R-32"]
["","Količina","","","kg","2.45","2.60","2.60","2.90"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675","675","675"]
["","Količina","","","tCO2Eq","1.65","1.76","1.76","1.96"]
["Povezivanje cevi","Tečnost","","SP","mm","9.52","9.52","9.52","9.52"]
["","Gas","","SP","mm","15.9","15.9","15.9","15.9"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","30","30","30","30"]
["","","Sistem","Odgovarajuća","m","50","50","50","50"]
["","","","Bez punjenja","m","30","30","30","30"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","Pogledati priručnik za instalaciju","Pogledati priručnik za instalaciju","Pogledati priručnik za instalaciju","Pogledati priručnik za instalaciju"]
["","Razlika nivoa","IU - OU","Maks.","m","30.0","30.0","30.0","30.0"]
["","","IU - IU","Maks.","m","0.5","0.5","0.5","0.5"]
["Standardni pribor","Installation manual","","","","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240"]
["Struja - 50Hz","Struja - 50Hz-=-Maksimalna amperaža osigurača (MFA)-=-A","","","A","20","25","32","32"]
["Standardni pribor","Peel off F-gas label","","","","1"]
["Beleške","","","","","","","(1) - U skladu sa ENER Lot 21","(1) - U skladu sa ENER Lot 21"]