{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000678"]
[]
[]
[]
[]
["","","","","","BR00000678."]
["Primena","","","","","Podni tip"]
["Kapacitet","m³/min","","","","33.33"]
["Kućište","Boja","","","","Završna obrada od obojenog galvanizovana čelika"]
["Dimenzije","Uređaj","","Visina","mm","1628"]
["","","","Širina","mm","720"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","770"]
["Težina","Uređaj","","","kg","150"]
["Primenljiva površina prostorije","m²","","","","133"]
["Prečišćavanje vazduha","Ulazna snaga","","H","kW","0.379"]
["Nivo zvučnog pritiska","Prečišćavanje vazduha","","Visok","dBA","55.9"]
["Ventilator","Brzina protoka vazduha","Prečišćavanje vazduha","Turbo","m³/h","2300"]
["","","","Visok","m³/h","2000"]
["Sigurnosni uređaji","Stavka","","01","","Sigurnosni prekidač (rad se zaustavlja kad su zadnja vrata otvorena)"]
["Standardni pribor","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Električni kabl","m","","","","3"]
["Izvor napajanja","Frekvencija","","","Hz","50/60"]
["Radna struja","Prečišćavanje vazduha","","Visok","A","1.73"]