{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":10,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 4MXM-A"]
[]
[]
[]
[]
["","","","","","CHYHBH05AFV32 / 4MXM68A2V1B","CHYHBH05AAV32 / 4MXM68A2V1B","CHYHBH05AFV32 / 4MXM80A2V1B","CHYHBH05AAV32 / 4MXM80A2V1B","CHYHBH08AAV32 / 4MXM80A2V1B"]
["Zagrevanje vode za domaćinstvo","Opšti podaci","","Deklarisani profil opterećenja","","XL","","XL"]
["","Prosečni klimatski uslovi","","Klasa energetske efikasnosti zagrevanja vode","","A","","A"]
["COP","","","","","3.91 (1)","3.91 (1)","4.04 (1)","4.04 (1)","4.17"]
["Grejanje prostora","Izlazna voda pri prosečnim klimatskim uslovima 55°C","Opšti podaci","Seasonal space heating eff. class","","A+","","A+"]
["","","","ηs (Sezonska efikasnost grejanja prostora)","%","113.3","","120.8"]
["","","","SCOP","","2.91","","3.09"]
["Kapacitet grejanja","Nom.","","","kW","4.50 (1)","","4.50 (1)"]
["Beleške","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), bojler premošćen","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), bojler premošćen","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), bojler premošćen","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), bojler premošćen","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), bojler premošćen"]
["Kapacitet grejanja","Nom.","","","kW","","4.5 (1)","","4.5 (1)","6.78"]
["Zagrevanje vode za domaćinstvo","Opšti podaci","","Deklarisani profil opterećenja","","","XL","","XL","XL"]
["","Prosečni klimatski uslovi","","Klasa energetske efikasnosti zagrevanja vode","","","A","","A","A"]
["Grejanje prostora","Izlazna voda pri prosečnim klimatskim uslovima 55°C","Opšti podaci","SCOP","","","2.91","","3.09","3.09"]
["","Izl. voda pri prosečnim klimatskim usl. 55°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","","A+","","A+","A+"]