{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Nivo zvučnog pritiska","Grejanje","Visok","dBA","39"]
["","","Srednji","dBA","32"]
["","","Nečujan rad","dBA","21"]
["","","Nizak","dBA","25"]
["","Hlađenje","Medium","dBA","32"]
["","","Nečujan rad","dBA","21"]
["","","Nizak","dBA","25"]
["","","Visok","dBA","39"]
["Standardni pribor","Priručnik za instalaciju","","","1"]
["","Priručnik za upotrebu","","","1"]
["","Filter za vazduh","","","2"]
["","Infracrveni daljinski upravljač","","","1"]
["","Noseća ploča daljinskog upravljača","","","1"]
["","Vreća za zavrtnje","","","1"]
["","Poklopac zavrtnja","","","1"]
["","AAA suve baterije","","","2"]
["","Opšta upozorenja u vezi sa bezbednošću","","","1"]
["Rashladno sredstvo","GWP (potencijal globalnog otopljavanja)","","","675.0"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Cevne spojnice","Tečnost","SP","mm","6.35"]
["","Gas","SP","mm","9.50"]
["","Ispusni otvor","","","18"]
["Apsorbovana snaga","Hlađenje","Nom.","kW","0.020"]
["","Grejanje","Nom.","kW","0.020"]
["Sound power level","Hlađenje","","dBA","57"]
["Dimenzije","Uređaj","Širina","mm","798"]
["","","Dubina","mm","189"]
["","","Visina","mm","295"]
["Kućište","Boja","","","Abonos"]
["Težina","Uređaj","","kg","12"]
["Power supply","Faza","","","1~"]
["","Frekvencija","","Hz","50"]
["","Ime","","","V1"]
["","Napon","","V","220-240"]