{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","38","","41"]
["","","","Nečujan rad","dBA","21","","21"]
["","","","Nizak","dBA","28","","30"]
["","Hlađenje","","Nečujan rad","dBA","21","","21"]
["","","","Nizak","dBA","25","","28"]
["","","","Visok","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Hlađenje","","Nom.","dBA","31","","35"]
["Standardni pribor","Priručnik za instalaciju","","","","1","","1"]
["","Priručnik za upotrebu","","","","1","","1"]
["","Bežični daljinski upravljač","","","","1","","1"]
["","Baterije","","","","2","","2"]
["","Držač daljinskog upravljača","","","","1","","1"]
["","Noseća ploča","","","","1","","1"]
["","Pričvrsni zavrtnji unutrašnje jedinice","","","","2","","2"]
["","Fotokatalitički filter za vazduh od titanijumapatita","","","","2","","2"]
["Kontrolni sistemi","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Piping connections","Tečnost","","SP","mm","6.35","","6.35"]
["","Gas","","SP","mm","9.5","","9.5"]
["","Ispusni otvor","","","","18","","18"]
["Apsorbovana snaga","Hlađenje","","Nom.","kW","0.040","","0.040"]
["","Grejanje","","Nom.","kW","0.040","","0.040"]
["Nivo zvučne snage","Hlađenje","","","dBA","55","","59"]
["","Grejanje","","","dBA","56","","58"]
["Dimenzije","Uređaj","","Širina","mm","780","","780"]
["","","","Dubina","mm","215","","215"]
["","","","Visina","mm","289","","289"]
["Kućište","Colour","","","","Bela","","Bela"]
["Težina","Uređaj","","","kg","8","","8"]
["Ventilator","Brzina protoka vazduha","Grejanje","Visok","m³/min","","","10.1"]
["","","","Nizak","m³/min","","","6.3"]
["","","","Nečujan rad","m³/min","","","4.3"]
["","","Hlađenje","Nizak","m³/min","","","5.2"]
["","","","Visok","m³/min","","","9.2"]
["","","","Nečujan rad","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Hlađenje","Nom.","m³/min","","","7.2"]
["Power supply","Phase","","","","1~","","1~"]
["","Frekvencija","","","Hz","50","","50"]
["","Ime","","","","V1","","V1"]
["","Napon","","","V","220-240","","220-240"]
["Beleške","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Ulazna snaga","Hlađenje","","Nom.","kW","","0.04","","0.040"]
["","Grejanje","","Nom.","kW","","0.04","","0.040"]
["Kućište","Boja","","","","","Bela","","Bela"]
["Dimenzije","Uređaj","","Visina","mm","","289","","289"]
["","","","Širina","mm","","780","","780"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","215","","215"]
["Težina","Uređaj","","","kg","","8","","8.00"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","","7.9","","9.2"]
["","","","Srednji","m³/min","","6.3","","7.2"]
["","","","Nizak","m³/min","","4.7","","5.2"]
["","","","Nečujan rad","m³/min","","3.9","","3.9"]
["","","Grejanje","Visok","m³/min","","9","","10.1"]
["","","","Srednji","m³/min","","7.5","","8.1"]
["","","","Nizak","m³/min","","6","","6.3"]
["","","","Nečujan rad","m³/min","","4.3","","4.3"]
["Nivo zvučne snage","Hlađenje","","","dBA","","55","","59"]
["","Grejanje","","","dBA","","56","","58"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","","37","","42"]
["","","","Srednji","dBA","","31","","35"]
["","","","Nizak","dBA","","25","","28"]
["","","","Nečujan rad","dBA","","21","","21"]
["","Grejanje","","Visok","dBA","","38","","41"]
["","","","Srednji","dBA","","33","","36"]
["","","","Nizak","dBA","","28","","30"]
["","","","Nečujan rad","dBA","","21","","21"]
["Povezivanje cevi","Tečnost","","SP","mm","","6.35","","6.35"]
["","Gas","","SP","mm","","9.5","","9.50"]
["","Ispusni otvor","","","","","18","","18"]
["Kontrolni sistemi","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Standardni pribor","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Napajanje","Ime","","","","","V1","","V1"]
["","Faza","","","","","1~","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","","50","","50"]
["","Napon","","","V","","220-240","","220-240"]