{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCS601C51"]
[]
[]
[]
[]
["","","","","","DCS601C51."]
["Ulaz","Tip","","","","Senzorska tabla (10 bita kodiranog analognog ulaza)"]
["Temperatura sredine","Relativna vlažnost <","","","%","85"]
["","Rad","","Min.","°C","0"]
["","","","Maks.","°C","40"]
["Maksimalan broj unutrašnjih jedinica koje je moguće priključiti:","","","","","64, 128 (1)"]
["Veza","DIII-NET","","Količina","","1"]
["","","","Napomena","","Vod za komunikaciju sa opremom za klimatizaciju"]
["","10BASE-T","","Napomena","","Opcija za web"]
["","Ethernet","","Napomena","","Portal za pristup internetu i funkcija e-pošte"]
["","Ulazni terminal","Digitalno","Količina","","1"]
["","","","Napomena","","Prisilno gašenje"]
["","","Impuls","Količina","","3"]
["","","","Napomena","","Impus za merenje napajanja"]
["","Modem","","Napomena","","Mogućnost ugrađivanja modema"]
["","PCMCIA","","Napomena","","Kartica za fleš memoriju"]
["","RS-232C","","Napomena","","DIII-NET PLUS adapter"]
["Dimenzije","Uređaj","","Širina","mm","230"]
["","","","Dubina","mm","107"]
["","","","Visina","mm","147"]
["LCD","Tip","","","","QVGA (320 x 240), 4.096 boje"]
["","Dimenzije","","širina","inča","5.7"]
["Maksimalan broj spoljašnjih jedinica koje je moguće priključiti","","","","","10, 20 (1)"]
["Power supply","Frekvencija","","","Hz","50/60"]
["","Napon","","","V","100-240 (sa spoljašnjim napajanjem)"]
["Beleške","","","","","(1) - U kombinaciji sa DCS601A51"]