{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-CB / ERHQ-BW17"]
[]
[]
[]
[]
["","","","","","EHBH16CB3V / ERHQ014BAW17","EHBH16CB9W / ERHQ014BAW17"]
["COP","","","","","4.24 (1), 3.22 (2)","4.24 (1), 3.22 (2)"]
["Kapacitet grejanja","Nom.","","","kW","14.5 (1), 13.6 (2)"]
["Apsorbovana snaga","Grejanje","","Nom.","kW","3.42 (1), 4.21 (2)"]
["Beleške","","","","","(1) - Uslov 1: hlađenje Ta 35°C - LWE 18℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Uslov 1: hlađenje Ta 35°C - LWE 18℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]
["","","","","","(3) - Tamb 35°C - LWE 7°C (DT=5°C)","(3) - Tamb 35°C - LWE 7°C (DT=5°C)"]
["","","","","","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)"]
["","","","","","(5) - DB/WB 7°C/6°C-LWC 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C-LWC 35°C(DT=5°C)"]
["","","","","","(6) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["Kapacitet grejanja","Nom.","","","kW","","14.5 (1), 13.6 (2)"]
["Ulazna snaga","Grejanje","","Nom.","kW","","3.42 (1), 4.21 (2)"]
["Grejanje prostora","Izlazna voda pri prosečnim klimatskim uslovima 55°C","Opšti podaci","SCOP","","","2.86"]
["","Izl. voda pri prosečnim klimatskim usl. 55°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","","A+"]
["","Izlazna voda pri prosečnim klimatskim uslovima 35°C","Opšti podaci","SCOP","","","3.34"]
["","Izl. voda pri prosečnim klimatskim usl. 35°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","","A+"]
["Opseg energetske efikasnosti","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]