{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-E / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHSH04P30EF / ERGA04EAV3","EHSH04P30EG / ERGA04EAV3"]
["Unutrašnja jedinica","","","","","EHSH04P30EF","EHSH04P30EG"]
["Kapacitet grejanja","Nom.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)"]
["Ulazna snaga","Grejanje","","Nom.","kW","0.840 (1), 1.26 (2)","0.840 (1), 1.26 (2)"]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)"]
["Zagrevanje vode za domaćinstvo","Opšti podaci","","Deklarisani profil opterećenja","","L","L"]
["","Prosečni klimatski uslovi","","Klasa energetske efikasnosti zagrevanja vode","","A+","A+"]
["Grejanje prostora","Izlazna voda pri prosečnim klimatskim uslovima 55°C","Opšti podaci","SCOP","","3.26","3.26"]
["","Izl. voda pri prosečnim klimatskim usl. 55°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","A++","A++"]
["","Izlazna voda pri prosečnim klimatskim uslovima 35°C","Opšti podaci","SCOP","","4.48","4.48"]
["","Izl. voda pri prosečnim klimatskim usl. 35°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","A+++","A+++"]
["Beleške","","","","","(1) - Uslov 1: hlađenje Ta 35°C - LWE 18℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Uslov 1: hlađenje Ta 35°C - LWE 18℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]
["Opseg energetske efikasnosti","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]