{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3"]
[]
[]
[]
[]
["","","","","","EHSX04P30DA3","EHSX04P50DA3","EHSX08P30DA3","EHSX08P50DA3"]
["Kućište","Boja","","","","Bela (RAL9016) / Tamno siva (RAL7011)","Bela (RAL9016) / Tamno siva (RAL7011)","Bela (RAL9016) / Tamno siva (RAL7011)","Bela (RAL9016) / Tamno siva (RAL7011)"]
["","Materijal","","","","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar"]
["Dimenzije","Uređaj","","Visina","mm","1891","1896","1891","1896"]
["","","","Širina","mm","595","790","595","790"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","615","790","615","790"]
["Težina","Uređaj","","","kg","73.0","93.0","73.0","93.0"]
["PED (Direktiva o opremi pod pritiskom)","Kategorija","","","","član 3.3","član 3.3","član 3.3","član 3.3"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32","R-32"]
["","GWP (potencijal globalnog otopljavanja)","","","","675.0","675.0","675.0","675.0"]
["","Količina","","","kg","1.50","1.50","1.50","1.50"]
["Nivo zvučne snage","Nom.","","","dBA","39","39","39","39"]
["Radni opseg","Grejanje","Vodeno kolo","Min.","°C","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65"]
["","Hlađenje","Spolja","Min.","°CDB","10","10","10","10"]
["","","Vodeno kolo","Min.","°C","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","230","230","230","230"]
["Električni grejač","Izvor napajanja","","Ime","","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Faza","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Frekvencija","Hz","50","50","50","50"]
["Beleške","","","","","(1) - Gubici toplote u skladu sa EN12897","(1) - Gubici toplote u skladu sa EN12897","(1) - Gubici toplote u skladu sa EN12897","(1) - Gubici toplote u skladu sa EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","","(5) - Zagrevanje rezervoara samo pomoću toplotne pumpe, bez elektr. grejača","","(5) - Zagrevanje rezervoara samo pomoću toplotne pumpe, bez elektr. grejača"]