{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-E"]
[]
[]
[]
[]
["","","","","","EHSXB04P30EG","EHSXB04P50EG","EHSXB08P30EG","EHSXB08P50EG","EHSXB04P30EF (Archived)","EHSXB04P50EF (Archived)","EHSXB08P30EF (Archived)","EHSXB08P50EF (Archived)"]
["Kućište","Boja","","","","bela (RAL9016) / crna (RAL9017)","bela (RAL9016) / crna (RAL9017)","bela (RAL9016) / crna (RAL9017)","bela (RAL9016) / crna (RAL9017)","bela (RAL9016) / crna (RAL9017)","bela (RAL9016) / crna (RAL9017)","bela (RAL9016) / crna (RAL9017)","bela (RAL9016) / crna (RAL9017)"]
["","Materijal","","","","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar"]
["Dimenzije","Uređaj","","Visina","mm","1891","1910","1891","1910","1892","1905","1892","1905"]
["","","","Širina","mm","594","792","594","792","594","792","594","792"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","644","817","644","817","644","812","644","812"]
["Težina","Uređaj","","","kg","80.0","104","80.0","104","79","110","79","110"]
["PED (Direktiva o opremi pod pritiskom)","Kategorija","","","","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP (potencijal globalnog otopljavanja)","","","","675.0","675.0","675.0","675.0","675","675","675","675"]
["","Količina","","","kg","1.50","1.50","1.50","1.50","1.5","1.5","1.5","1.5"]
["Nivo zvučne snage","Nom.","","","dBA","39","39","39","39","39","39","39","39"]
["Radni opseg","Grejanje","Vodeno kolo","Min.","°C","18","18","18","18","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65","65","65","65","65"]
["","Hlađenje","Spolja","Min.","°CDB","10","10","10","10","10","10","10","10"]
["","","Vodeno kolo","Min.","°C","5","5","5","5","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22","22","22","22","22"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50","50","50","50","50"]
["","Napon","","","V","230","230","230","230","230","230","230","230"]
["Beleške","","","","","(1) - Gubici toplote u skladu sa EN12897","(1) - Gubici toplote u skladu sa EN12897","(1) - Gubici toplote u skladu sa EN12897","(1) - Gubici toplote u skladu sa EN12897","(1) - Gubici toplote u skladu sa EN12897","(1) - Gubici toplote u skladu sa EN12897","(1) - Gubici toplote u skladu sa EN12897","(1) - Gubici toplote u skladu sa EN12897"]