{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-E9W / ERGA-EVH"]
[]
[]
[]
[]
["","","","","","EHVZ08S18EA9W / ERGA06EAV3H","EHVZ08S18EJ9W / ERGA06EAV3H","EHVZ08S23EA9W / ERGA06EAV3H","EHVZ08S23EJ9W / ERGA06EAV3H"]
["Kapacitet grejanja","Nom.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)"]
["Ulazna snaga","Grejanje","","Nom.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)"]
["Apsorbovana snaga","Topla sanitarna voda od 10°C do 50°C","","Nom.","kWh","2.48","2.48","3.01","3.01"]
["Vreme zagrevanja od 10°C do 50°C","sati","","","","1h28min","1h28min","1h40min","1h40min"]
["COP","","","","","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)"]
["Zagrevanje vode za domaćinstvo","Opšti podaci","","Deklarisani profil opterećenja","","L","L","XL","XL"]
["","Prosečni klimatski uslovi","","Klasa energetske efikasnosti zagrevanja vode","","A+","A+","A+","A+"]
["Grejanje prostora","Izlazna voda pri prosečnim klimatskim uslovima 55°C","Opšti podaci","SCOP","","3.26","3.26","3.26","3.26"]
["","Izl. voda pri prosečnim klimatskim usl. 55°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","A++","A++","A++","A++"]
["","Izlazna voda pri prosečnim klimatskim uslovima 35°C","Opšti podaci","SCOP","","4.47","4.47","4.47","4.47"]
["","Izl. voda pri prosečnim klimatskim usl. 35°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","A+++","A+++","A+++","A+++"]
["Opseg energetske efikasnosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Beleške","","","","","(1) - Uslov 1: hlađenje Ta 35°C - LWE 18℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Uslov 1: hlađenje Ta 35°C - LWE 18℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Uslov 1: hlađenje Ta 35°C - LWE 18℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Uslov 1: hlađenje Ta 35°C - LWE 18℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]