{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELBH-E9W / ERRA08-12EW1"]
[]
[]
[]
[]
["","","","","","ELBH12EF9W / ERRA08EAW1","ELBH12EF9W / ERRA10EAW1","ELBH12EF9W / ERRA12EAW1"]
["Kapacitet grejanja","Min.","","","kW","3.45","3.45","3.45"]
["","Nom.","","","kW","6.17","6.17","6.17"]
["","Maks.","","","kW","7.95","9.25","9.97"]
["Ulazna snaga","Grejanje","","Min.","kW","0.70","0.70","0.70"]
["","","","Nom.","kW","1.21","1.21","1.21"]
["","","","Maks.","kW","1.63","1.98","2.21"]
["COP","","","","","5.10","5.10","5.10"]
["Grejanje prostora","Izlazna voda pri prosečnim klimatskim uslovima 55°C","Opšti podaci","SCOP","","3.42","3.43","3.53"]
["","Izl. voda pri prosečnim klimatskim usl. 55°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","A++","A++","A++"]
["","Izlazna voda pri prosečnim klimatskim uslovima 35°C","Opšti podaci","SCOP","","4.81","4.84","4.84"]
["","Izl. voda pri prosečnim klimatskim usl. 35°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","A+++","A+++","A+++"]
["Beleške","","","","","(1) - Kapacitet prema standardu EN14511 i validno za opseg zagrevane vode dT = 3~8°C pri Ta 7°C","(1) - Kapacitet prema standardu EN14511 i validno za opseg zagrevane vode dT = 3~8°C pri Ta 7°C","(1) - Kapacitet prema standardu EN14511 i validno za opseg zagrevane vode dT = 3~8°C pri Ta 7°C"]
["","","","","","(2) - Uslov: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uslov: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uslov: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Apsorbovana snaga je ukupna snaga unutrašnjih i spoljašnjih jedinica, uključujući i cirkulacionu pumpu; u skladu sa EN14511","(3) - Apsorbovana snaga je ukupna snaga unutrašnjih i spoljašnjih jedinica, uključujući i cirkulacionu pumpu; u skladu sa EN14511","(3) - Apsorbovana snaga je ukupna snaga unutrašnjih i spoljašnjih jedinica, uključujući i cirkulacionu pumpu; u skladu sa EN14511"]
["","","","","","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) maksimalna brzina pumpe","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) maksimalna brzina pumpe","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) maksimalna brzina pumpe"]