{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELBX-E9W"]
[]
[]
[]
[]
["","","","","","ELBX12EF9W"]
["Kućište","Boja","","","","Belo + crno"]
["","Materijal","","","","Smola, metalna ploča"]
["Dimenzije","Uređaj","","Visina","mm","840"]
["","","","Širina","mm","440"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","390"]
["Težina","Uređaj","","","kg","48.5"]
["PED (Direktiva o opremi pod pritiskom)","Kategorija","","","","Kategorija II"]
["Nivo zvučne snage","Nom.","","","dBA","44.0 (3)"]
["Nivo zvučnog pritiska","Nom.","","","dBA","30.0 (4)"]
["Radni opseg","Grejanje","Vodeno kolo","Min.","°C","15 (5)"]
["","","","Maks.","°C","65 (5)"]
["","Hlađenje","Spolja","Min.","°CDB","10 (5)"]
["","","Vodeno kolo","Min.","°C","5 (5)"]
["","","","Maks.","°C","22 (5)"]
["Napajanje","Ime","","","","Pogledajte napomenu 6"]
["Električni grejač","Izvor napajanja","","Ime","","9W"]
["","","","Faza","","3~"]
["","","","Frekvencija","Hz","50"]
["","","","Napon","V","400"]
["","Preporučena veličina","","","A","20.000 (7)"]
["Beleške","","","","","(1) - Radno područje je prošireno na niže brzine protoka zavisno od režima rada - pogledati ESP krivu."]
["","","","","","(2) - Isključujući zapreminu vode u uređaju. Ova količina vode garantuje dovoljnu energiju za odmrzavanje pri bilo kojoj primeni, ali može biti umnožena sa 0,66 ako je granična temperatura ≥ 45° C ( na pr. ventilator-konvektori)"]
["","","","","","(3) - Meren uz pad pritiska od 10 kPa u sistemu grejanja i uz radni uslov koji zahteva da temperatura izlazne vode iznosi 47-55°C, u prostoriji u kojoj okolna temperatura iznosi 20°C. DB/WB 7°C/6°."]
["","","","","","(4) - Vrednosti zvuka se mere u polugluvoj sobi. Nivo zvučnog pritiska je relativna vrednost koja zavisi od rastojanja i akustike okolnog prostora. Za više informacija pogledajte dijagrame nivoa zvuka. Nivo zvučne snage je apsolutna vrednost koju stvara zvuk."]
["","","","","","(5) - Za dodatne informacije, pogledajte šemu radnih opsega"]
["","","","","","(6) - Gore pomenuti modul za napajanje hidrauličnog bloka služi samo za rezervni grejač. Komandna tabla i pumpa hidro modula se isporučuju sa spoljnim uređajem. Izborni rezervoar za domaću vruću vodu ima poseban izvor napajanja."]
["","","","","","(7) - 4 polni 20 A zakrivljeni 400 V otvarač klase C (pogledajte dijagram ožičenja)"]
["","","","","","(8) - Odaberite prečnik i vrstu spoja u skladu sa nacionalnim i lokalnim propisima"]