{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":11,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSX-E / ERRA-EV37"]
[]
[]
[]
[]
["","","","","","ELSX12P50EG / ERRA08EAV37","ELSX12P30EG / ERRA08EAV37","ELSX12P50EG / ERRA10EAV37","ELSX12P30EG / ERRA10EAV37","ELSX12P30EG / ERRA12EAV37","ELSX12P50EG / ERRA12EAV37"]
["Unutrašnja jedinica","","","","","ELSX12P50EG","ELSX12P30EG","ELSX12P50EG","ELSX12P30EG","ELSX12P30EG","ELSX12P50EG"]
["Kapacitet grejanja","Min.","","","kW","3.45 (1)","3.45 (1)","3.45 (1)","3.45 (1)","3.45 (1)","3.45 (1)"]
["","Nom.","","","kW","6.17 (2)","6.17 (2)","6.17 (2)","6.17 (2)","6.17 (2)","6.17 (2)"]
["","Maks.","","","kW","7.95 (1)","7.95 (1)","9.25 (1)","9.25 (1)","9.97 (1)","9.97 (1)"]
["Kapacitet hlađenja","Nom.","","","kW","6.81 (3), 6.47 (4)","6.81 (3), 6.47 (4)","7.97 (3), 6.47 (4)","7.97 (3), 6.47 (4)","8.62 (3), 6.47 (4)","8.62 (3), 6.47 (4)"]
["Ulazna snaga","Grejanje","","Min.","kW","0.72 (5)","0.72 (5)","0.72 (5)","0.72 (5)","0.72 (5)","0.72 (5)"]
["","","","Nom.","kW","1.25 (2)","1.25 (2)","1.25 (2)","1.25 (2)","1.25 (2)","1.25 (2)"]
["","","","Maks.","kW","1.69 (5)","1.69 (5)","2.04 (5)","2.04 (5)","2.28 (5)","2.28 (5)"]
["","Hlađenje","","Nom.","kW","2.15 (3), 1.16 (4)","2.15 (3), 1.16 (4)","2.66 (3), 1.16 (4)","2.66 (3), 1.16 (4)","2.96 (3), 1.16 (4)","2.96 (3), 1.16 (4)"]
["Apsorbovana snaga","Topla sanitarna voda od 10°C do 50°C","","Nom.","kWh","4.82 (6)","3.57 (6)","4.82 (6)","3.57 (6)","3.57 (6)","4.82 (6)"]
["Vreme zagrevanja od 10°C do 50°C","sati","","","","3 h 45 min","2 h 29 min","3 h 45 min","2 h 29 min","2 h 29 min","3 h 45 min"]
["COP","","","","","4.92 (2)","4.92 (2)","4.92 (2)","4.92 (2)","4.92 (2)","4.92 (2)"]
["EER","","","","","3.17 (3), 5.56 (4)","3.17 (3), 5.56 (4)","3.00 (3), 5.56 (4)","3.00 (3), 5.56 (4)","2.91 (3), 5.56 (4)","2.91 (3), 5.56 (4)"]
["Zagrevanje vode za domaćinstvo","Opšti podaci","","Deklarisani profil opterećenja","","XL","L","XL","L","L","XL"]
["","Prosečni klimatski uslovi","","Klasa energetske efikasnosti zagrevanja vode","","A+","A+","A+","A+","A+","A+"]
["Grejanje prostora","Izlazna voda pri prosečnim klimatskim uslovima 55°C","Opšti podaci","SCOP","","3.58","3.58","3.58","3.58","3.58","3.58"]
["","Izl. voda pri prosečnim klimatskim usl. 55°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","A++","A++","A++","A++","A++","A++"]
["","Izlazna voda pri prosečnim klimatskim uslovima 35°C","Opšti podaci","SCOP","","4.79","4.79","4.82","4.82","4.82","4.82"]
["","Izl. voda pri prosečnim klimatskim usl. 35°C","Opšti podaci","Klasa sezonske efikasnosti grejanja prostora","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Opseg energetske efikasnosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Beleške","","","","","(1) - Kapacitet prema standardu EN14511 i validno za opseg zagrevane vode dT = 3~8°C pri Ta 7°C","(1) - Kapacitet prema standardu EN14511 i validno za opseg zagrevane vode dT = 3~8°C pri Ta 7°C","(1) - Kapacitet prema standardu EN14511 i validno za opseg zagrevane vode dT = 3~8°C pri Ta 7°C","(1) - Kapacitet prema standardu EN14511 i validno za opseg zagrevane vode dT = 3~8°C pri Ta 7°C","(1) - Kapacitet prema standardu EN14511 i validno za opseg zagrevane vode dT = 3~8°C pri Ta 7°C","(1) - Kapacitet prema standardu EN14511 i validno za opseg zagrevane vode dT = 3~8°C pri Ta 7°C"]
["","","","","","(2) - Uslov: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uslov: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uslov: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uslov: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uslov: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Uslov: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Hlađenje: EW 12°C; LW 7°C; spoljni uslovi: 35°CDB","(3) - Hlađenje: EW 12°C; LW 7°C; spoljni uslovi: 35°CDB","(3) - Hlađenje: EW 12°C; LW 7°C; spoljni uslovi: 35°CDB","(3) - Hlađenje: EW 12°C; LW 7°C; spoljni uslovi: 35°CDB","(3) - Hlađenje: EW 12°C; LW 7°C; spoljni uslovi: 35°CDB","(3) - Hlađenje: EW 12°C; LW 7°C; spoljni uslovi: 35°CDB"]
["","","","","","(4) - Hlađenje: EW 23°C; LW 18°C; spoljni uslovi: 35°CDB","(4) - Hlađenje: EW 23°C; LW 18°C; spoljni uslovi: 35°CDB","(4) - Hlađenje: EW 23°C; LW 18°C; spoljni uslovi: 35°CDB","(4) - Hlađenje: EW 23°C; LW 18°C; spoljni uslovi: 35°CDB","(4) - Hlađenje: EW 23°C; LW 18°C; spoljni uslovi: 35°CDB","(4) - Hlađenje: EW 23°C; LW 18°C; spoljni uslovi: 35°CDB"]
["","","","","","(5) - Apsorbovana snaga je ukupna snaga unutrašnjih i spoljašnjih jedinica, uključujući i cirkulacionu pumpu; u skladu sa EN14511","(5) - Apsorbovana snaga je ukupna snaga unutrašnjih i spoljašnjih jedinica, uključujući i cirkulacionu pumpu; u skladu sa EN14511","(5) - Apsorbovana snaga je ukupna snaga unutrašnjih i spoljašnjih jedinica, uključujući i cirkulacionu pumpu; u skladu sa EN14511","(5) - Apsorbovana snaga je ukupna snaga unutrašnjih i spoljašnjih jedinica, uključujući i cirkulacionu pumpu; u skladu sa EN14511","(5) - Apsorbovana snaga je ukupna snaga unutrašnjih i spoljašnjih jedinica, uključujući i cirkulacionu pumpu; u skladu sa EN14511","(5) - Apsorbovana snaga je ukupna snaga unutrašnjih i spoljašnjih jedinica, uključujući i cirkulacionu pumpu; u skladu sa EN14511"]
["","","","","","(6) - Test na Ta DB/WB 7°C/6°C. U skladu sa EN 16147.","(6) - Test na Ta DB/WB 7°C/6°C. U skladu sa EN 16147.","(6) - Test na Ta DB/WB 7°C/6°C. U skladu sa EN 16147.","(6) - Test na Ta DB/WB 7°C/6°C. U skladu sa EN 16147.","(6) - Test na Ta DB/WB 7°C/6°C. U skladu sa EN 16147.","(6) - Test na Ta DB/WB 7°C/6°C. U skladu sa EN 16147."]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) maksimalna brzina pumpe","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) maksimalna brzina pumpe","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) maksimalna brzina pumpe","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) maksimalna brzina pumpe","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) maksimalna brzina pumpe","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) maksimalna brzina pumpe"]