{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSX-E"]
[]
[]
[]
[]
["","","","","","ELSX12P30EG","ELSX12P50EG","ELSX12P30EF (Archived)","ELSX12P50EF (Archived)"]
["Kućište","Boja","","","","bela (RAL9016) / crna (RAL9017)","bela (RAL9016) / crna (RAL9017)","bela (RAL9016) / crna (RAL9017)","bela (RAL9016) / crna (RAL9017)"]
["","Materijal","","","","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar","Polipropilen otporan na udar"]
["Dimenzije","Uređaj","","Visina","mm","1891","1910","1893","1910"]
["","","","Širina","mm","594","792","594","792"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","680","817","680","817"]
["Težina","Uređaj","","","kg","91.0","112","76.0","91.0"]
["PED (Direktiva o opremi pod pritiskom)","Kategorija","","","","Kategorija II","Kategorija II","Kategorija II","Kategorija II"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32","R-32"]
["Nivo zvučne snage","Nom.","","","dBA","44.7","44.7","44.7","44.7"]
["Nivo zvučnog pritiska","Nom.","","","dBA","36.8","36.8","36.8","36.8"]
["Radni opseg","Grejanje","Vodeno kolo","Min.","°C","15 (3)","15 (3)","15 (3)","15 (3)"]
["","","","Maks.","°C","65 (3)","65 (3)","65 (3)","65 (3)"]
["","Hlađenje","Spolja","Min.","°CDB","10 (3)","10 (3)","10 (3)","10 (3)"]
["","","Vodeno kolo","Min.","°C","5 (3)","5 (3)","5 (3)","5 (3)"]
["","","","Maks.","°C","22 (3)","22 (3)","22 (3)","22 (3)"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","230","230","230","230"]
["Beleške","","","","","(1) - Radno područje je prošireno na niže brzine protoka zavisno od režima rada - pogledati ESP krivu.","(1) - Radno područje je prošireno na niže brzine protoka zavisno od režima rada - pogledati ESP krivu.","(1) - Radno područje je prošireno na niže brzine protoka zavisno od režima rada - pogledati ESP krivu.","(1) - Radno područje je prošireno na niže brzine protoka zavisno od režima rada - pogledati ESP krivu."]
["","","","","","(2) - Gubici toplote u skladu sa EN12897","(2) - Gubici toplote u skladu sa EN12897","(2) - Gubici toplote u skladu sa EN12897","(2) - Gubici toplote u skladu sa EN12897"]
["","","","","","(3) - Za dodatne informacije, pogledajte šemu radnih opsega","(3) - Za dodatne informacije, pogledajte šemu radnih opsega","(3) - Za dodatne informacije, pogledajte šemu radnih opsega","(3) - Za dodatne informacije, pogledajte šemu radnih opsega"]