{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERRA08-12EV3"]
[]
[]
[]
[]
["","","","","","ERRA08EAV3","ERRA10EAV3","ERRA12EAV3"]
["Dimenzije","Uređaj","","Visina","mm","1,003","1,003","1,003"]
["","","","Širina","mm","1270","1270","1270"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","533","533","533"]
["Težina","Uređaj","","","kg","107","107","107"]
["Ventilator","Brzina protoka vazduha","Grejanje","Visok","m³/min","89.9","89.9","89.9"]
["","","Hlađenje","Visok","m³/min","80.1","80.1","80.1"]
["Radni opseg","Hlađenje","","Min.","°CDB","10","10","10"]
["","","","Maks.","°CDB","43","43","43"]
["","Sanitarna topla voda","","Min.","°CDB","-25","-25","-25"]
["","Topla voda za domaćinstvo","","Maks.","°CDB","35","35","35"]
["Nivo zvučne snage","Grejanje","","Nom.","dBA","56.0","56.0","56.0"]
["","Hlađenje","","Nom.","dBA","60.1","60.6","61.5"]
["Nivo zvučnog pritiska","Grejanje","","Nom.","dBA","40.6","40.6","40.6"]
["","Hlađenje","","Nom.","dBA","47","47.4","48.5"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32"]
["","GWP (potencijal globalnog otopljavanja)","","","","675.0","675.0","675.0"]
["","Količina","","","tCO2Eq","2.19","2.19","2.19"]
["","Količina","","","kg","3.25","3.25","3.25"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35"]
["","Gas","","SP","mm","15.9","15.9","15.9"]
["Cevne spojnice","Razlika nivoa","IU - OU","Maks.","m","30.0","30.0","30.0"]
["Napajanje","Ime","","","","V3","V3","V3"]
["","Faza","","","","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","230","230","230"]
["Struja","Osigurači koji se preporučuju","","","A","32","32","32"]
["Beleške","","","","","(1) - Hlađenje Ta 35°C - LWE 18℃ (DT = 5℃); grejanje Ta DB/WB 7°C/6°C - LWC 35℃ (DT = 5°C)","(1) - Hlađenje Ta 35°C - LWE 18℃ (DT = 5℃); grejanje Ta DB/WB 7°C/6°C - LWC 35℃ (DT = 5°C)","(1) - Hlađenje Ta 35°C - LWE 18℃ (DT = 5℃); grejanje Ta DB/WB 7°C/6°C - LWC 35℃ (DT = 5°C)"]
["","","","","","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Uslov 2: hlađenje Ta 35°C - LWE 7℃ (DT = 5°C); grejanje Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]
["","","","","","(3) - Nivo zvučnog pritiska je relativna vrednost koja zavisi od rastojanja i akustike okolnog prostora. Za više informacija pogledajte dijagrame nivoa zvuka.","(3) - Nivo zvučnog pritiska je relativna vrednost koja zavisi od rastojanja i akustike okolnog prostora. Za više informacija pogledajte dijagrame nivoa zvuka.","(3) - Nivo zvučnog pritiska je relativna vrednost koja zavisi od rastojanja i akustike okolnog prostora. Za više informacija pogledajte dijagrame nivoa zvuka."]
["","","","","","(4) - Nivo zvučnog pritiska se meri mikrofonom na određenom rastojanju od uređaja. To je relativna vrednost koja zavisi od rastojanja i akustike okruženja. Za dodatne informacije pogledajte šemu zvučnog spektra. Uslovi: Ta 35°C - LWE 7°C ( DT = 5°C).","(4) - Nivo zvučnog pritiska se meri mikrofonom na određenom rastojanju od uređaja. To je relativna vrednost koja zavisi od rastojanja i akustike okruženja. Za dodatne informacije pogledajte šemu zvučnog spektra. Uslovi: Ta 35°C - LWE 7°C ( DT = 5°C).","(4) - Nivo zvučnog pritiska se meri mikrofonom na određenom rastojanju od uređaja. To je relativna vrednost koja zavisi od rastojanja i akustike okruženja. Za dodatne informacije pogledajte šemu zvučnog spektra. Uslovi: Ta 35°C - LWE 7°C ( DT = 5°C)."]