{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":14,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZAG-NY1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / RZAG71N2Y1B","FAA71BUV1B / RZAG71N7Y1B","FAA100BUV1B / RZAG71N2Y1B","FAA100BUV1B / RZAG71N7Y1B","FAA100BUV1B / RZAG100N2Y1B","FAA100BUV1B / RZAG100N7Y1B","FAA71BUV1B / FAA71BUV1B / RZAG100N2Y1B","FAA71BUV1B / FAA71BUV1B / RZAG100N7Y1B","FAA71BUV1B / FAA71BUV1B / RZAG140N2Y1B","FAA71BUV1B / FAA71BUV1B / RZAG140N7Y1B"]
["Kapacitet hlađenja","Nom.","","kW","6.80","6.80 (1)","","","9.50","9.50 (1)"]
["Hlađenje prostora","SEER","","","6.58","6.58","","","6.42","6.42"]
["","Godišnja potrošnja električne energije","","kWh/god.","362","362","","","518","518"]
["","Kapacitet","Pdesign","kW","6.80","6.80","","","9.50","9.50"]
["","Klasa energetske efikasnosti","","","A++","A++","","","A++","A++"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","4.70","4.70","","","7.80","7.80"]
["","SCOP/A","","","4.20","4.20","","","4.01","4.01"]
["","Klasa energetske efikasnosti","","","A+","A+","","","A+","A+"]
["","Godišnja potrošnja električne energije","","kWh/god.","1,567","1,567","","","2,725","2,723"]
["Nominalna efikasnost","EER","","","3.27","","","","3.24"]
["","Godišnja potrošnja električne energije","","kWh","1,040","","","","1,466"]
["","COP","","","3.42","","","","3.17"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","","","","A"]
["","","Grejanje","","B","","","","D"]
["Kapacitet grejanja","Nom.","","kW","7.50","7.50 (2)","","","10.80","10.8 (2)"]
["Beleške","","","","","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["Kapacitet hlađenja","Nom.","","kW","","","6.80 (1)","6.80 (1)","","","9.50 (1)","9.50 (1)","13.4 (1)","13.4 (1)"]
["Kapacitet grejanja","Nom.","","kW","","","7.50 (2)","7.50 (2)","","","10.8 (2)","10.8 (2)","15.5 (2)","15.5 (2)"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","","","A++","A++","","","A+++","A+++"]
["","Kapacitet","Pdesign","kW","","","6.80","6.80","","","9.50","9.50","13.4","13.4"]
["","SEER","","","","","6.43","6.43","","","8.57","8.57","8.18","8.18"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","370","370","","","388","388","982","982"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","","","A+","A+","","","A++","A++"]
["","Kapacitet","Pdesign","kW","","","4.70","4.70","","","7.80","7.80","9.52","9.52"]
["","SCOP/A","","","","","4.10","4.10","","","4.63","4.63","4.52","4.52"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","1605","1605","","","2359","2359","2946","2946"]
["Opseg energetske efikasnosti","","","","","","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]