{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Kućište","Boja","","","","Bela","Bela"]
["","Materijal","","","","Smola","Smola"]
["Dimenzije","Uređaj","","Visina","mm","290","340"]
["","","","Širina","mm","1050","1200"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","269","262"]
["Težina","Uređaj","","","kg","14","18"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","16.2","23"]
["","","","Srednji","m³/min","13.4","21.1"]
["","","","Nizak","m³/min","12.1","18.7"]
["","","Grejanje","Visok","m³/min","16.9","23"]
["","","","Srednji","m³/min","14.2","20.9"]
["","","","Nizak","m³/min","12.7","18.7"]
["Nivo zvučne snage","Hlađenje","","","dBA","61","65"]
["","Grejanje","","","dBA","61","65"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","45","49"]
["","","","Srednji","dBA","42","45"]
["","","","Nizak","dBA","40","41"]
["","Grejanje","","Visok","dBA","45","49"]
["","","","Srednji","dBA","42","45"]
["","","","Nizak","dBA","40","41"]
["Povezivanje cevi","Tečnost","","SP","mm","9.52","9.52"]
["","Gas","","SP","mm","15.9","15.9"]
["","Ispusni otvor","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Napajanje","Faza","","","","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]
["Standardni pribor","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Beleške","","","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["Standardni pribor","Screw cover","","","","","3"]