{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / 3MXM-A9"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / FBA35A2VEB9 / 3MXM68A2V1B9"]
["Kapacitet hlađenja","Nom.","","kW","6.80"]
["Kapacitet grejanja","Nom.","","kW","8.60"]
["Nominalna efikasnost","EER","","","2.73"]
["","COP","","","3.24"]
["","Godišnja potrošnja električne energije","","kWh","1245"]
["","Direktiva o energetskom označavanju","Hlađenje","","D"]
["","","Grejanje","","C"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A"]
["","Kapacitet","Pdesign","kW","6.80"]
["","SEER","","","5.42"]
["","Godišnja potrošnja električne energije","","kWh/god.","440"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A"]
["","Kapacitet","Pdesign","kW","3.60"]
["","SCOP/A","","","3.81"]
["","Pdh Kapacitet grejanja na -10°C","","kW","3.10"]
["","Godišnja potrošnja električne energije","","kWh/god.","1323"]