{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZQ-C"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZQ200C7Y1B","FBA60A2VEB9 / FBA60A2VEB9 / FBA60A2VEB9 / FBA60A2VEB9 / RZQ250C7Y1B"]
["Kapacitet hlađenja","Nom.","","kW","20.0 (1)","24.1 (1)"]
["Hlađenje prostora","SEER","","","5.67","5.74"]
["","Godišnja potrošnja električne energije","","kWh/a","2,115","2,518"]
["","Kapacitet","Pdesign","kW","20.0","24.1"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","11.2","12.1"]
["","SCOP/A","","","3.68","3.76"]
["","Godišnja potrošnja električne energije","","kWh/a","4,257","4,484"]
["Kapacitet grejanja","Nom.","","kW","23.0 (2)","26.4 (2)"]
["Beleške","","","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m"]
["","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m"]
["","","","","(3) - Ova vrednost ne uključuje smanjenje kapaciteta usled rada funkcije odmrzavanja.","(3) - Ova vrednost ne uključuje smanjenje kapaciteta usled rada funkcije odmrzavanja."]