{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":15,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZAG71M7V1B","FBA35A2VEB / FBA35A2VEB / RZAG71M7V1B","FBA50A2VEB / FBA50A2VEB / RZAG71M7V1B","FBA71A2VEB / RZAG71M7V1B","FBA50A2VEB / FBA50A2VEB / RZAG100M7V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZAG100M7V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZAG100M7V1B","FBA50A2VEB / FBA50A2VEB / FBA50A2VEB / RZAG100M7V1B","FBA71A2VEB / FBA71A2VEB / RZAG100M7V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZAG125M7V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZAG140M7V1B"]
["Kapacitet hlađenja","Nom.","","kW","6.80 (1)","6.80 (1)","6.80 (1)","6.80 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","","12.1 (1)","13.4 (1)"]
["Hlađenje prostora","Godišnja potrošnja električne energije","","kWh/god.","469","401","437","382","510","572","567","508","","649","699"]
["","Kapacitet","Pdesign","kW","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","","12.1","13.4"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","4.70","4.70","4.70","4.70","7.80","7.80","7.80","7.80","","9.52","9.52"]
["","Godišnja potrošnja električne energije","","kWh/god.","1,732","1,700","1,696","1,566","2,651","2,786","2,730","2,690","","2,240","3,332"]
["Kapacitet grejanja","Nom.","","kW","7.50 (2)","7.50 (2)","7.50 (2)","7.50 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","","13.5 (2)","15.5 (2)"]
["Hlađenje prostora","SEER","","","5.08","5.94","5.45","6.22","6.52","5.81","5.86","6.54","","11.2","11.5"]
["","Klasa energetske efikasnosti","","","B","A+","A","A++","A++","A+","A+","A++"]
["Grejanje prostora (Prosečna klima)","SCOP/A","","","3.80","3.87","3.88","4.20","4.12","3.92","4.00","4.06","","5.95","4.00"]
["","Klasa energetske efikasnosti","","","A","A","A","A+","A+","A","A","A+"]
["Beleške","","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Hlađenje: T2: unutrašnja temp. 26,6°CDB, 19,4 °CWB, spoljna temp. 48°CDB [Btu/hr/W]","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Hlađenje: T2: unutrašnja temp. 26,6°CDB, 19,4 °CWB, spoljna temp. 48°CDB [Btu/hr/W]","(1) - Hlađenje: T2: unutrašnja temp. 26,6°CDB, 19,4 °CWB, spoljna temp. 48°CDB [Btu/hr/W]","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Hlađenje: T2: unutrašnja temp. 26,6°CDB, 19,4 °CWB, spoljna temp. 48°CDB [Btu/hr/W]","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m"]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["Spoljni uređaj","","","","","","","","","","","","RZAG100M7V1B"]
["Kapacitet hlađenja","Nom.","","kW","","","","","","","","","9.50 (1)"]
["Kapacitet grejanja","Nom.","","kW","","","","","","","","","10.8 (2)"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","","","","","","","","","A++"]
["","Kapacitet","Pdesign","kW","","","","","","","","","9.50"]
["","SEER","","","","","","","","","","","7.88"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","","","","","","422"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","","","","","","","","","A+"]
["","Kapacitet","Pdesign","kW","","","","","","","","","7.80"]
["","SCOP/A","","","","","","","","","","","4.43"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","","","","","","2465"]
["Opseg energetske efikasnosti","","","","","","","","","","","","A+++ ~ D"]