{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FBA71A2VEB / RZASG71M2V1B","FBA35A2VEB / FBA35A2VEB / RZASG71M2V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZASG125M7V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZASG140M7V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZASG100M7V1B (Archived)","FBA50A2VEB / FBA50A2VEB / RZASG100M7V1B (Archived)"]
["Kapacitet hlađenja","Nom.","","kW","6.80 (1)","6.80 (1)"]
["Hlađenje prostora","SEER","","","6.19","5.43"]
["","Godišnja potrošnja električne energije","","kWh/god.","385","438"]
["","Kapacitet","Pdesign","kW","6.80","6.80"]
["","Klasa energetske efikasnosti","","","A++","A"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","4.50","4.50"]
["","SCOP/A","","","4.01","3.82"]
["","Klasa energetske efikasnosti","","","A+","A"]
["","Godišnja potrošnja električne energije","","kWh/god.","1,571","1,649"]
["Kapacitet grejanja","Nom.","","kW","7.50 (2)","7.50 (2)"]
["Beleške","","","","(1) - Hlađenje: T2: unutrašnja temp. 26,6°CDB, 19,4 °CWB, spoljna temp. 48°CDB [Btu/hr/W]","(1) - Hlađenje: T2: unutrašnja temp. 26,6°CDB, 19,4 °CWB, spoljna temp. 48°CDB [Btu/hr/W]","(1) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["Spoljni uređaj","","","","","","RZASG125M7V1B","RZASG140M7V1B","RZASG100M7V1B","RZASG100M7V1B"]
["Kapacitet hlađenja","Nom.","","kW","","","12.1","13.4","9.50","9.50"]
["Kapacitet grejanja","Nom.","","kW","","","13.5","15.5","10.8","10.8"]
["Hlađenje prostora","Kapacitet","Pdesign","kW","","","12.1","13.4","9.50","9.50"]
["","SEER","","","","","8.59","9.67","5.31","5.38"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","845","832","626","618"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","","","6.00","7.80","6.00","6.00"]
["","SCOP/A","","","","","5.09","5.62","3.80","3.80"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","1650","1943","2211","2211"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","","","","","A","A"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","","","","","A","A"]