{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50AVEB / RXS50L2V1B","FCAG60AVEB / RXS60L2V1B"]
["Kapacitet hlađenja","Nom.","","kW","5.00","5.70"]
["Space cooling","SEER","","","6.48","6.22"]
["","Godišnja potrošnja električne energije","","kWh/a","270","321"]
["","Kapacitet","Pdesign","kW","5.00","5.70"]
["","Klasa energetske efikasnosti","","","A++","A++"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","4.36","4.71"]
["","SCOP/A","","","4.29","4.00"]
["","Klasa energetske efikasnosti","","","A++","A+"]
["","Godišnja potrošnja električne energije","","kWh/a","1,426","1,646"]
["Cevne spojnice","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","12.70","12.70"]
["","Ispusni otvor","OD","mm","VP25 (Spoljni preč.32, unutrašnji preč. 25)","VP25 (Spoljni preč.32, unutrašnji preč. 25)"]
["Nominalna efikasnost","EER","","","3.55","3.48"]
["","Annual energy consumption","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","A","B"]
["Kapacitet grejanja","Nom.","","kW","6.00","7.00"]
["Beleške","","","","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]