{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXM-A9"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXM35A5V1B9","FCAG50BVEB / RXM50A5V1B9"]
["Kapacitet hlađenja","Nom.","","kW","3.5","5"]
["Kapacitet grejanja","Nom.","","kW","4.2","6"]
["Nominalna efikasnost","EER","","","3.72","3.58"]
["","COP","","","3.77","3.7"]
["","Godišnja potrošnja električne energije","","kWh","470","698"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","A","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A++","A++"]
["","Kapacitet","Pdesign","kW","3.5","5"]
["","SEER","","","6.51","6.54"]
["","Godišnja potrošnja električne energije","","kWh/god.","188","268"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A++","A+"]
["","Kapacitet","Pdesign","kW","3.32","4.36"]
["","SCOP/A","","","4.98","4.3"]
["","Pdh Kapacitet grejanja na -10°C","","kW","2.67","3.86"]
["","Godišnja potrošnja električne energije","","kWh/god.","933","1418"]
["Beleške","","","","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]