{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RXS50L2V1B","FCAG60BVEB / RXS60L2V1B"]
["Kapacitet hlađenja","Nom.","","kW","5.00","5.70"]
["Kapacitet grejanja","Nom.","","kW","6.00","7.00"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","EER","","","3.55","3.48"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","A","B"]
["Povezivanje cevi","Ispusni otvor","OD","mm","VP25 (Spoljni preč.32, unutrašnji preč. 25)","VP25 (Spoljni preč.32, unutrašnji preč. 25)"]
["","Gas","SP","mm","12.70","12.70"]
["","Tečnost","SP","mm","6.35","6.35"]
["Beleške","","","","(1) - Pri normalnom radu: +22°C / +32°C","(1) - Pri normalnom radu: +22°C / +32°C"]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]