{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZA-D"]
[]
[]
[]
[]
["","","","","FCAG60BVEB / FCAG60BVEB / FCAG60BVEB / RZA200D7Y1B","FCAG71BVEB / FCAG71BVEB / FCAG71BVEB / RZA200D7Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZA200D7Y1B","FCAG60BVEB / FCAG60BVEB / FCAG60BVEB / FCAG60BVEB / RZA250D7Y1B","FCAG125BVEB / FCAG125BVEB / RZA250D7Y1B","FCAG100BVEB / FCAG100BVEB / RZA200D7Y1B (Archived)"]
["Kapacitet hlađenja","Nom.","","kW","19.0 (1)","19.0 (1)","19.0 (1)","22.0 (1)","22.0 (1)"]
["Kapacitet grejanja","Nom.","","kW","22.4 (2)","22.4 (2)","22.4 (2)","24.0 (2)","24.0 (2)"]
["Hlađenje prostora","Kapacitet","Pdesign","kW","19.0","19.0","19.0","22.0","22.0"]
["","SEER","","","6.77","6.32","7.16","6.95","6.44"]
["","Godišnja potrošnja električne energije","","kWh/god.","1,684","1,804","1,592","1,898","2,052"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","11.2","11.2","11.2","12.1","12.1"]
["","SCOP/A","","","3.84","4.10","4.10","4.10","4.10"]
["","Godišnja potrošnja električne energije","","kWh/god.","4,082","3,824","3,825","4,132","4,132"]
["Beleške","","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["Kapacitet hlađenja","Nom.","","kW","","","","","","19.0 (1)"]
["Kapacitet grejanja","Nom.","","kW","","","","","","22.4 (2)"]
["Hlađenje prostora","Kapacitet","Pdesign","kW","","","","","","19.0"]
["","SEER","","","","","","","","6.53"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","","","1746"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","","","","","","11.2"]
["","SCOP/A","","","","","","","","4.10"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","","","3824"]