{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQSG100L8Y1B","FCAHG125GVEB / RZQSG125L8Y1B","FCAHG140GVEB / RZQSG140L7Y1B"]
["Kapacitet hlađenja","Nom.","","kW","9.50 (1)","12.0 (1)","13.4 (1)"]
["Hlađenje prostora","SEER","","","6.70","5.40"]
["","Godišnja potrošnja električne energije","","kWh/a","497","778"]
["","Kapacitet","Pdesign","kW","9.50","12.0"]
["","Klasa energetske efikasnosti","","","A++","A"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","8.03","8.03"]
["","SCOP/A","","","4.30","4.10"]
["","Klasa energetske efikasnosti","","","A+","A+"]
["","Godišnja potrošnja električne energije","","kWh/a","2,615","2,742"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","1,285","1,855"]
["","EER","","","3.70 (3)","3.23 (3)","3.11 (3)"]
["","COP","","","4.30 (3)","3.75 (3)","3.61 (3)"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","A","A"]
["Kapacitet grejanja","Nom.","","kW","10.8 (2)","13.5 (2)","15.5 (2)"]
["Beleške","","","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m"]
["","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m"]
["","","","","(3) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(3) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(3) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]