{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-J"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXS35J2V1B","FCQG50FVEB / RXS50J2V1B"]
["Kapacitet hlađenja","Nom.","","kW","3.40 (3)","5.00 (3)"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","475","705"]
["","EER","","","3.58","3.55"]
["","COP","","","3.41","3.70"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","B","A"]
["Kapacitet grejanja","Nom.","","kW","4.20 (4)","6.00 (4)"]
["Beleške","","","","(1) - Energetska oznaka: skala od A (najefikasnije) do G (najmanja efikasnost)","(1) - Energetska oznaka: skala od A (najefikasnije) do G (najmanja efikasnost)"]
["","","","","(2) - Godišnja potrošnja energije: na osnovi prosečne upotrebe od 500 radnih časova godišnje pod punim opterećenjem (nominalni uslovi)","(2) - Godišnja potrošnja energije: na osnovi prosečne upotrebe od 500 radnih časova godišnje pod punim opterećenjem (nominalni uslovi)"]
["","","","","(3) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m","(3) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m"]
["","","","","(4) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5 m; visinska razlika: 0m","(4) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5 m; visinska razlika: 0m"]
["","","","","(5) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(5) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]